Time Stamping Button

Tutorial:

Copy script “timeTool.sh” to location “home/pi/Documents/bash/”

Copy “autostart” file to “home/pi/.config/lxsession/LXDE-pi/”

Open File home/pi/.bashrc

Insert @lxterminal

Save and close

Open Browser go to muster\_company.biral.ch and login. When browser ask to save login credential click ok

Connect Hardware button between GND and GPIO 7

Reset Pi and you are ready to go